| Flutter Impeller |

Classes | Public Types | Public Member Functions | Static Public Member Functions | List of all members
impeller::android::HardwareBuffer Class Reference

A wrapper for AHardwareBuffer https://developer.android.com/ndk/reference/group/a-hardware-buffer. More...

`#include <hardware_buffer.h>`

## Public Types
enum class | CPUAccessType { kRead , kWrite }

## Public Member Functions
| HardwareBuffer (HardwareBufferDescriptor descriptor)
| ~HardwareBuffer ()
| HardwareBuffer (const HardwareBuffer &)=delete
HardwareBuffer & | operator= (const HardwareBuffer &)=delete
bool | IsValid () const
AHardwareBuffer * | GetHandle () const
const HardwareBufferDescriptor & | GetDescriptor () const
const AHardwareBuffer_Desc & | GetAndroidDescriptor () const
std::optional< uint64_t > | GetSystemUniqueID () const
| Get the system wide unique ID of the hardware buffer if possible. This is only available on Android API 31 and above. Within the process, the handle are unique. More...
void * | Lock (CPUAccessType type) const
| Lock the buffer for CPU access. This call may fail if the buffer was not created with one the usages that allow for CPU access. More...
bool | Unlock () const
| Unlock a mapping previously locked for CPU access. More...

## Static Public Member Functions
static bool | IsAvailableOnPlatform ()
static std::optional< AHardwareBuffer_Desc > | Describe (AHardwareBuffer *buffer)
static std::optional< uint64_t > | GetSystemUniqueID (AHardwareBuffer *buffer)
| Get the system wide unique ID of the hardware buffer if possible. This is only available on Android API 31 and above. Within the process, the handle are unique. More...

## Detailed Description

A wrapper for AHardwareBuffer https://developer.android.com/ndk/reference/group/a-hardware-buffer.

This wrapper creates and owns a handle to a managed hardware buffer. That is, there is no ability to take a reference to an externally created hardware buffer.

This wrapper is only available on Android API 29 and above.

Definition at line 95 of file hardware_buffer.h.

## Member Enumeration Documentation

## ◆ CPUAccessType

enum impeller::android::HardwareBuffer::CPUAccessType
| strong

Enumerator
kRead |
kWrite |

Definition at line 135 of file hardware_buffer.h.

135 {
136 kRead,
137 kWrite,
138 };

## Constructor & Destructor Documentation

## ◆ HardwareBuffer() [1/2]

impeller::android::HardwareBuffer::HardwareBuffer | ( | HardwareBufferDescriptor | descriptor | ) |
| explicit

Definition at line 57 of file hardware_buffer.cc.

58 : descriptor_(descriptor),
59 android_descriptor_(ToAHardwareBufferDesc(descriptor_)) {
60 if (!descriptor_.IsAllocatable()) {
61 VALIDATION_LOG << "The hardware buffer descriptor is not allocatable.";
62 return;
63 }
64 const auto& proc_table = GetProcTable();
65
66 AHardwareBuffer* buffer = nullptr;
67 if (auto result =
68 proc_table.AHardwareBuffer_allocate(&android_descriptor_, &buffer);
69 result != 0 || buffer == nullptr) {
70 VALIDATION_LOG << "Could not allocate hardware buffer. Error: " << result;
71 return;
72 }
73 buffer_.reset(buffer);
74 is_valid_ = true;
75 }
impeller::android::GetProcTable
const ProcTable & GetProcTable()
Definition: proc_table.cc:12
impeller::android::ToAHardwareBufferDesc
static AHardwareBuffer_Desc ToAHardwareBufferDesc(const HardwareBufferDescriptor &desc)
Definition: hardware_buffer.cc:20
impeller::android::HardwareBufferDescriptor::IsAllocatable
bool IsAllocatable() const
If hardware buffers can be created using this descriptor. Allocatable descriptors may still cause fai...
Definition: hardware_buffer.cc:52
VALIDATION_LOG
#define VALIDATION_LOG
Definition: validation.h:91

References impeller::android::GetProcTable(), impeller::android::HardwareBufferDescriptor::IsAllocatable(), and VALIDATION_LOG.

## ◆ ~HardwareBuffer()

impeller::android::HardwareBuffer::~HardwareBuffer | ( |  | ) |
| default

## ◆ HardwareBuffer() [2/2]

impeller::android::HardwareBuffer::HardwareBuffer | ( | const HardwareBuffer & |  | ) |
| delete

## Member Function Documentation

## ◆ Describe()

std::optional< AHardwareBuffer_Desc > impeller::android::HardwareBuffer::Describe | ( | AHardwareBuffer * | buffer | ) |
| static

Definition at line 127 of file hardware_buffer.cc.

128 {
129 if (!buffer || !GetProcTable().AHardwareBuffer_describe) {
130 return std::nullopt;
131 }
132 AHardwareBuffer_Desc desc = {};
133 GetProcTable().AHardwareBuffer_describe(buffer, &desc);
134 return desc;
135 }

References impeller::android::GetProcTable().

Referenced by impeller::android::testing::TEST().

## ◆ GetAndroidDescriptor()

const AHardwareBuffer_Desc & impeller::android::HardwareBuffer::GetAndroidDescriptor | ( |  | ) | const

Definition at line 103 of file hardware_buffer.cc.

103 {
104 return android_descriptor_;
105 }

## ◆ GetDescriptor()

const HardwareBufferDescriptor & impeller::android::HardwareBuffer::GetDescriptor | ( |  | ) | const

Definition at line 99 of file hardware_buffer.cc.

99 {
100 return descriptor_;
101 }

## ◆ GetHandle()

AHardwareBuffer * impeller::android::HardwareBuffer::GetHandle | ( |  | ) | const

Definition at line 83 of file hardware_buffer.cc.

83 {
84 return buffer_.get();
85 }

Referenced by impeller::glvk::CreateEGLImageFromAHBTexture(), GetSystemUniqueID(), impeller::android::SurfaceTransaction::SetContents(), and impeller::android::testing::TEST().

## ◆ GetSystemUniqueID() [1/2]

std::optional< uint64_t > impeller::android::HardwareBuffer::GetSystemUniqueID | ( |  | ) | const

Get the system wide unique ID of the hardware buffer if possible. This is only available on Android API 31 and above. Within the process, the handle are unique.

Returns
  The system unique id if one can be obtained.

Definition at line 111 of file hardware_buffer.cc.

111 {
112 return GetSystemUniqueID(GetHandle());
113 }
impeller::android::HardwareBuffer::GetHandle
AHardwareBuffer * GetHandle() const
Definition: hardware_buffer.cc:83
impeller::android::HardwareBuffer::GetSystemUniqueID
std::optional< uint64_t > GetSystemUniqueID() const
Get the system wide unique ID of the hardware buffer if possible. This is only available on Android A...
Definition: hardware_buffer.cc:111

References GetHandle().

Referenced by impeller::android::testing::TEST().

## ◆ GetSystemUniqueID() [2/2]

std::optional< uint64_t > impeller::android::HardwareBuffer::GetSystemUniqueID | ( | AHardwareBuffer * | buffer | ) |
| static

Get the system wide unique ID of the hardware buffer if possible. This is only available on Android API 31 and above. Within the process, the handle are unique.

Returns
  The system unique id if one can be obtained.

Definition at line 115 of file hardware_buffer.cc.

116 {
117 if (!GetProcTable().AHardwareBuffer_getId) {
118 return std::nullopt;
119 }
120 uint64_t out_id = 0u;
121 if (GetProcTable().AHardwareBuffer_getId(buffer, &out_id) != 0) {
122 return std::nullopt;
123 }
124 return out_id;
125 }

References impeller::android::GetProcTable().

## ◆ IsAvailableOnPlatform()

bool impeller::android::HardwareBuffer::IsAvailableOnPlatform | ( |  | ) |
| static

Definition at line 107 of file hardware_buffer.cc.

107 {
108 return GetProcTable().IsValid() && GetProcTable().AHardwareBuffer_isSupported;
109 }
impeller::android::ProcTable::IsValid
bool IsValid() const
If a valid proc table could be setup. This may fail in case of setup on non-Android platforms.
Definition: proc_table.cc:65

References impeller::android::GetProcTable(), and impeller::android::ProcTable::IsValid().

Referenced by impeller::AHBSwapchainVK::IsAvailableOnPlatform(), and impeller::android::testing::TEST().

## ◆ IsValid()

bool impeller::android::HardwareBuffer::IsValid | ( |  | ) | const

Definition at line 79 of file hardware_buffer.cc.

79 {
80 return is_valid_;
81 }

Referenced by impeller::android::testing::TEST().

## ◆ Lock()

void * impeller::android::HardwareBuffer::Lock | ( | CPUAccessType | type | ) | const

Lock the buffer for CPU access. This call may fail if the buffer was not created with one the usages that allow for CPU access.

Parameters

  [in] | type | The type

Returns
  A host-accessible buffer if there was no error related to usage or buffer validity.

Definition at line 137 of file hardware_buffer.cc.

137 {
138 if (!is_valid_ || !GetProcTable().AHardwareBuffer_lock) {
139 return nullptr;
140 }
141 uint64_t usage = 0;
142 switch (type) {
143 case CPUAccessType::kRead:
144 usage |= AHARDWAREBUFFER_USAGE_CPU_READ_MASK;
145 break;
146 case CPUAccessType::kWrite:
147 usage |= AHARDWAREBUFFER_USAGE_CPU_WRITE_MASK;
148 break;
149 }
150 void* buffer = nullptr;
151 const auto result = GetProcTable().AHardwareBuffer_lock( //
152 buffer_.get(), // buffer
153 usage, // usage
154 -1, // fence
155 nullptr, // rect
156 &buffer // out-addr
157 );
158 return result == 0 ? buffer : nullptr;
159 }
type
GLenum type
Definition: blit_command_gles.cc:153
impeller::android::HardwareBuffer::CPUAccessType::kRead
@ kRead
impeller::android::HardwareBuffer::CPUAccessType::kWrite
@ kWrite

References impeller::android::GetProcTable(), kRead, kWrite, and type.

## ◆ operator=()

HardwareBuffer& impeller::android::HardwareBuffer::operator= | ( | const HardwareBuffer & |  | ) |
| delete

## ◆ Unlock()

bool impeller::android::HardwareBuffer::Unlock | ( |  | ) | const

Unlock a mapping previously locked for CPU access.

Returns
  If the unlock was successful.

Definition at line 161 of file hardware_buffer.cc.

161 {
162 if (!is_valid_ || !GetProcTable().AHardwareBuffer_unlock) {
163 return false;
164 }
165 const auto result =
166 GetProcTable().AHardwareBuffer_unlock(buffer_.get(), nullptr);
167 return result == 0;
168 }

References impeller::android::GetProcTable().

The documentation for this class was generated from the following files:

- impeller/toolkit/android/hardware_buffer.h
- impeller/toolkit/android/hardware_buffer.cc